National University of Computer and Emerging Sciences 

**Laboratory Manual**

*for*

**Computer Organization and Assembly Language Programming**

| Course Instructor | Aleena Ahmad |
| --- | --- |
| Lab Instructor | Sana Ejaz |
| Semester | Fall 2024 |

Department of Computer Science

FAST-NU, Lahore, Pakistan

Page 1

**OBJECTIVES:**

∙ How to manipulate display memory by writing a single character on the screen at a specific location in video memory.

∙ How to display background color and change intensity.

∙ How to display String on a specific location.

∙ How to move a string from one location in memory to another.

**Instructions:**

| **1. Submit work in a single Word file with screenshots of meaningful results. 2. Press F2 if you want to step over the function Call. F1 will step into the function.**  **3. Use DOSBox's memory viewer to check the video memory. You can access video memory starting from 0xB800 to see the changes made by your program.** |
| --- |

**Command to run: > nasm -f bin -o myprogram.com myprogram.asm > myprogram.com**

**Task 1: Write a program to place the character 'A' at the top-left corner of the screen (row 0, column 0).**

**a)** Display the character 'A' with white text on a blue background.


**b)** Display 'A' with a Blue Background and Increased Intensity of white text.

**(a)**

| [org 0x0100]  MOV AX, 0xB800  MOV ES, AX  MOV word [ES:00], 0x1741  MOV AX, 0x4C00  INT 0x21 |
| --- |


**(b)**

| [org 0x0100]  MOV AX, 0xB800  MOV ES, AX  MOV word [ES:00], 0x1F41  MOV AX, 0x4C00  INT 0x21 |
| --- |

****

**Task 2: Write a program to display "HELLO" starting at the second row (row 1), and third column (column 2). Use white text on a black background.**

| [org 0x0100]  JMP start  msg: db 'HELLO'  size: dw 5  printstr:  PUSH BP  MOV BP, SP  PUSHA  MOV AX, 0xB800  MOV ES, AX    MOV CX, [BP + 4]  MOV SI, [BP + 6]  MOV DI, 164  lop1:  MOV AL, [SI]  MOV AH, 0x07  MOV [ES:DI], AX  INC SI  ADD DI, 2  LOOP lop1  POPA  MOV SP, BP  POP BP  RET 4  start:  PUSH word msg  PUSH word [size]  CALL printstr  MOV AX, 0x4C00  INT 0x21 |
| --- |

****

**Task 3: Write a Program to Fill Memory with a Character Using STOS**

| [org 0x0100]  MOV AX, 0xB800  MOV ES, AX  MOV AX, 0x0741  MOV CX, 2000  MOV DI, 0  REP STOSW  MOV AX, 0x4C00  INT 0x21 |
| --- |

